TOC · Work · Menu · Drive · Device I/O Parameters Device I/O Dialog Box

### Device I/O Handler Script

The script can be used for I/O error logging and for extended processing of errors (include external program calls). The feature is available in the Professional Edition only.

Script can be loaded or modified via Device I/O Parameters (button Script).

The file ondevhsc.txt contains a brief description of available commands and some script examples.

Possible script lines are of the form:
IF CONDITION COMMAND
or
COMMAND
or
:LABEL
where CONDITION is an inequality or equality (!=, >, <, >=, <=, =) of two quantities,
and quantity is either an integer constant (0, 1, ...) or a variable (the list is below) or a simple mathematical expression (operators +, -, *, %, /, without parentheses, ignoring the mathematical order of operators), e.g. %ERROR%=0
Comments are preceded by two minuses (--)

#### Variables

Zero based

%CONFIRM% | =1 if Confirm pressed, =0 if Cancel pressed (confirmation dialog box appears)
%DISKNUM% | disk number in RAID array
%TRYNUM% | i/o retry number
%LBA% | first i/o sector number
%SECNUM% | number of i/o sectors
%ERROR% | i/o error
%ATASTATUS% | ATA Status Register value (defined if BSY bit is cleared, DOS ATA only)
%ATAERROR% | ATA Error Register (defined if ERR bit of %ATASTATUS% is set)
%LINE% | current line number in script
%SERVICE% | i/o service: 0-ATA 1-ATAPI 3-BIOSINT13OLD 4-BIOSINT13 5-DOSINT25 6-DOSINT73 8-DOSMSCDEX 9-DOSFILE 11-WINFILE 12-WINSCSI 14-WIN9XINT13 20-LINUXFILE
%LASTRES% | result of the previous command
%LASTERR% | error of the previous command

#### Commands

SHOWDLG - force device i/o dialog box popping up
WAIT - wait for user choice
DELAY N - delay for N msec
EXECCMD CMDLINE - execute external command CMDLINE using Command interpreter (equals "cmd CMDLINE" in Windows)
EXECCMDQ CMDLINE - execute without creating new console window (quiet)
EXEC "FILENAME" CMDLINE - call external programm FILENAME with parameter CMDLINE
EXECQ "FILENAME" CMDLINE - call without creating new console window (quiet)
MSDOS - call Command processor (not supported in Linux)
GOTO LABELNAME - jump to label LABELNAME in script (to the string :LABELNAME)
RETURN - break script execution, handle error according to device I/O params
RETRETRY - break script as Retry button pressed
RETIGNORE - break script as Ignore button pressed
RETABORT - break script as Abort button pressed
ADDLOG "FILENAME" LOGLINE - write LOGLINE to file FILENAME (string LOGLINE may contain variables)
CANCELIO - Call CancelIO (WinNT+ only) (available if a device is opened with overlapped option)
OVLRESLT N - Check Overlapped result (N=1: wait; N=0: not wait) (WinNT+ only) (must be used if a device is opened with overlapped option)
RESETHANDLE - Reopen disk handle (WinNT+ only)
ATARESET - ATA Soft Reset (DOS ATA only)
ATARESETDET - ATA Soft Reset followed by ATA Identify (DOS ATA only)

#### Format specifiers

-- To format output integer a variable name may be followed
-- by a format specifier after a colon, e.g.
-- %LBA:8x% - width: 8, hexadecimal

#### Sample

IF %ERROR%=0 RETURN -- return if no error on last i/o
IF %ERROR%=128 GOTO LABEL1
IF %ERROR%=5 GOTO LABEL1
RETURN
:LABEL1
IF %CONFIRM%=0 RETRETRY -- retry if Cancel button is pressed
-- continue script execution if Confirm is pressed
EXECCMD /K ECHO error %ERROR% at LBA: %LBA% (%SECNUM%) try: %TRYNUM%. Type EXIT to return.
IF %TRYNUM%<2 RETRETRY
DELAY 500
ADDLOG "C:\ERRORS.LOG" error %ERROR:x% at LBA: %LBA:10% (%SECNUM%) try: %TRYNUM%
RETIGNORE